# ID 70405

The telegram element configured for the #DRIVE command is used exclusively from the CNC.
Description | The telegram element configured for bitwise writing (P-AXIS-00398) in a drive function is used exclusively by the CNC. See also: [PROG// Section: Drive-independent switching of drive functions]
Response | Class | 1 | Error message output, evaluation of drive functions is aborted.
Solution | Class | 1 | P-AXIS-00398 value must be adjusted.
Parameter | %1: | Logical axis number [-]
%2: | Current value [-]
Name of the configured drive function (P-AXIS-00396).
%3: | Error value [-]
Configured value of P-AXIS-00398
Error type | -