# Manual activation (P-COMP-00029)

P-COMP-00029 | Manual activation
Description | Cross compensation is automatically activated by the CNC if it selected in the axis parameters (P-AXIS-00047) and the required conditions are met (e.g. axis is homed). If the parameter is set to the value 1, cross compensation must be activated explicitly by an NC command (see [PROG//Selecting/deselecting axis compensations in the NC program]. In addition, compensation is deselected at the end of the NC program, at CNC reset and on axis release.
Parameter | kw.crosscomp.manual_activation
Data type | BOOLEAN
Data range | 0: Automatic activation 1: Manual activation in NC program
Axis types | T, R, S
Dimension | T: ---- | R,S: ----
Default value | 0
Remarks |