# ID 21303

Automatic determination of feed coupling factor without selection not allowed.
Description | When programming Spindle feed link, the keyword AUTO was programmed without ON or OFF. Example: Wrong: N10 G00 X0 Y0 Z0 N20 S[FEED_LINK AUTO]

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. The keyword AUTO only may be programmed in combination with ON or OFF. Example: Correct: N10 G00 X0 Y0 Z0 N20 S[FEED_LINK ON AUTO]

:

N1000 M30

Error type | 1, Error message from NC program.