# ID 110126

Maximum velocity for manual mode exceeds limit.
Description | The maximum velocity P-AXIS-00213 in active manual mode is greater than the maximum value. The maximum velocity is set to default value.
Response | Class | 1 | None.
Solution | Class | 1 | Set maximum velocity for manual mode P-AXIS-00213 to smaller than maximum value P-AXIS-00212.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [1µm/s or 0.001°/s]
Current maximum velocity P-AXIS-00213.
%3: | Limit value [1µm/s or 0.001°/s]
Upper limit value of velocity.
%4: | Corrected value [1µm/s or 0.001°/s]
Corrected maximum velocity P-AXIS-00213.
Error type | 2, Error message on data transfer of parameter lists to controller.