# ID 70490

The Volumetric Compensation cannot be updated, because no memory has been allocated.
Description | The parameter update of the compensation failed, since no memory has been allocated for it during controller start-up, see P-STUP-00100.
Response | Class | 3 |
Solution | Class | 6 | Adjust P-STUP-00100, restart the controller.
Parameter | %1: | Compensation index [-]
ID of volumetric compensation
Error type | 11, Error message from position controller.