# ID 120564

The minimum block length for dynamic segmentation is smaller than permissible minimum value.
Description | The HSC value specified in the channel list for the minimum block length of relevant blocks P-CHAN-00140 (see: hsc.gen.min_segment_length in [0.1um]) was too small. Blocks below this length are not specified in finer resolution in the dynamic consideration.
Response | Class | 1 | Warning
Solution | Class | 1 | Value is limited to minimum
Parameter | %1: | Current value [0.1 µm or 0.0001°]
%2: | Limit value [0.1 µm or 0.0001°]
%3: | Corrected value [0.1 µm or 0.0001°]
Error type |