# ID 110342

Axis number for gantry master axis has to be 0.
Description | The axis is marked as the master axis of a gantry combination in the parameter P-AXIS-00015. At the same time, this axis has an entry for a leading master axis P-AXIS-00070. This is not permitted.
Response | Class | 3 | Abort current job.
Solution | Class | 7 | The entry of the logical axis number P-AXIS-00070 must be assigned 0 in the master axis of the gantry combination.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Logical axis number [-]
Current entry of the logical axis number for P-AXIS-00070.
%3: | Corrected value [-]
New entry for P-AXIS-00070
Error type | 2, Error message by data transfer from parameter list into control device.