# Response to maximum tracked axis deviation (P-CHAN-00130)

P-CHAN-00130 | Response to maximum tracked axis deviation (B Spline)
Description | This parameter defines which measure is used for B spline generation when the maximum tracked axis deviation is exceeded.
Parameter | hsc.bspline.auto_off_track
Data type | BOOLEAN
Data range | 0: The B spline is reduced (corner distance is reduced) in order to maintain the predefined maximum deviation and the B spline touches the original path before and after the corner. The B spline is not deselected. 1: The B spline is automatically deselected at the corner. Therefore, any contour bend at the corner is retained.
Dimension | ----
Default value | 0
Remarks |