# ID 110391

2nd proportional gain of the dynamic gain adjustment is initialized with 0.
Description | The second proportional gain P-AXIS-00247 of the dynamic Kv-adjustment was given as 0. This is an invalid value.
Response | Class | 1 | Element is initialized by default value.
Solution | Class | 1 | Correct parameter list of axis.
Parameter | %1: | Logical axis number [-]
P-AXIS-00016
%2: | Current value [-]
P-AXIS-00247
%3: | Corrected value [-]
P-AXIS-00247
Error type | 2, Error message by data transfer from parameter list into control device.