# ID 50601

Invalid command after Sync. OUT.
Description | The target position after #SYNC OUT is programmed as an independent axis which can be interrupted by following #SYNC IN command: <axis_name>[INDP_SYN … POS<value> INTERRUPTIBLE]
Response | Class | 6 |
Solution | Class | 6 |
Parameter | %1: | Current value [-]
%2: | Expected value [-]
%3: | Current value [-]
%4: | Block number [-]
Error type | 1, Error message from NC program.