# ID 110229

Logical axis number in compensation data list and in command-PDU not equal.
Description | A logical axis should use a compensation value list. Therefore this list is interpreted. While interpreting it is detected, that the number of the logical axis of the compensation value list isn’t that number of the logical axis that should use this list.
Response | Class | 3 | Abort interpretation of the compensation value list.
Solution | Class | 7 | Check which compensation value list is to be used for the axis. May be you have to change the number of the logical axis in the list or have to use another list.
Parameter | %1: | Current value [-]
Number of a logical axis. This number (P-COMP-00001) comes from the compensation value list that should be used.
%2: | Expected value [-]
Number of the logical axis to be used by the compensation value list (P-STUP-00036).
Error type | -