# ID 70523

Permissible distance for movement from reference cam exceeded.
Description | During homing, the maximum covered distance set in P-AXIS-00531 was exceeded when moving away from the reference cam. Possible causes for this error message are:

- the reference switch is ‘frozen’.
- P-AXIS-00531 setting is too small.

Response | Class | 7 | Error message output, abort NC program.
Solution | Class | 6 | Possible remedies:

- Check reference switch function
- Set larger parameter in P-AXIS-00531

Parameter | %1: | Logical axis number [-]
Logical axis number (P-AXIS-00016) of affected axis
%2: | Error value [-]
Distance covered on moving away from cam
%3: | Limit value [-]
Maximum permissible distance
%4: | Current value [-]
Current command position
Error type | 11, Error message from position controller.