# ID 50050

Probing cycle not initialized.
Description | When using the measurement function G100, different measurement types can be completely contoured in the measurement block.. For preparation of probe hardware the measurement process in CNC is activated in previous movement block. The initialization of probe hardware has to be finished before moving in measure movement block.

For detailed information on measurement function G100, FCT-C4], [PROG// Section: Measuring functions].

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Either use measurement type with motion stop or reduce delay time before initialization of probe hardware.
Parameter | %1: | Block number [-]
%2: | Current value [-]
Error type | 1, Error message from NC program.