# ID 50067

No motion information available.
Description | With the measurement function G100, a relevant motion path must be programmed. Wrong: %mess N10 G00 X100 Y0 Z100 N20 G100 X100 F2000

N30 M30

Correct:

%mess

N10 G00 X100 Y0 Z0

N20 G100 X200 F2000

N30 M30

For detailed information on G100, see[FCT-C4], [PROG// Section: Measuring functions].

Response | Class | 4 | Movement stop.
Solution | Class | 6 | Measurement movement block with path > 0
Error type | 1, Error message from NC program.