# Overview

Constant | Description
M_FKT_ANZ | Maximum number of M functions [SYSP, Section "System parameters CNC"]
KANAL_ANZ_RND | Maximum number of independent channels [SYSP, Section "System parameters CNC"]

ID | Meaning
--- | ---
P-STUP-00033 | Memory size for backward motion
P-CHAN-00041 | Synchronisation types for M functions
P-CHAN-00275 | Backward motion with offset
P-CHAN-00276 | Programmed M00 stop during backward motions
P-CHAN-00277 | Programmed M00 stop during next forward motions
P-CHAN-00278 | Programmed M01 stop during backward movement
P-CHAN-00279 | Programmed M01 stop during next forward movement
P-CHAN-00308 | Response at STOP marks during forward movement
P-CHAN-00309 | Response at STOP marks during repeated forward movement
P-CHAN-00310 | Response at STOP marks during backward movement