# Block selection in the case of linear segmentation (P-CHAN-00133)

P-CHAN-00133 | Number of blocks for linear segmentation (HSC)
Description | This parameter defines the number of blocks which are generated during linear segmentation. Set the parameter P-CHAN-00134 to 0. Depending on the block motion path available, 4 or 3 block segments are generated. In both cases, the segments at the start and end of the block have the length P-CHAN-00135. If the block motion path is not long enough (shorter than 3* P-CHAN-00135), the original motion path is split into two blocks.
Parameter | hsc.gen.linear_center_point
Data type | BOOLEAN
Data range | 0: 3 block segments where the first and last segment P-CHAN-00135 are long and the middle segment has the length of the distance to go. 1: 4 block segments where the first and last segment P-CHAN-00135 are long and the middle two segments share the distance to go.
Dimension | ----
Default value | 1
Remarks |