# ID 21259

Too many axes requested.
Description | For the channel more axes are requested, than in the channel are permissible at all.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the axis exchange command . Request fewer axes or rethink program concept. There is no way to exchanged more axes into a NC channel, than the system limits allow.
Parameter | %1: | Error value [-]
Current number of requested axes.
%2: | Upper limit value [-]
Maximum permissible number of axes in the channel. Version-specific setting [SYSP].
Error type | 1, Error message from NC program.