# ID 20385

Coordinate is out of data format.
Description | When calculating the axis positions after deselection of synchronous operation, or after deselection of a coordinate transformation, it is determined that an axis position exceeds the permissible value range.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check the machine axis positions before deselecting synchronous operation or coordinate transformation. Move to a smaller axis position in the NC program before deselecting this option. Check whether the correct kinematic type is entered in the channel parameters P-CHAN-00032 or in the NC program (#KIN ID).
Parameter | %1: | Error value [-]
%2: | Lower limit value [-]
%3: | Upper limit value [-]
Error type | 1, Error message from NC program.