# Maximum time for drive reset (P-AXIS-00484)

P-AXIS-00484 | Maximum time for drive reset
Description | By default an error message is output when the reset of a drive amplifier takes longer than 20 seconds. During this time the CNC axis can not be used. This parameter defines the time until output of the error message. Here a minimum value of 100000 µs is allowed.

If P-AXIS-00484 is less than this minimum value warning, P-ERR-110562 is output and the parameter is set to the minimum value.

Parameter | antr.reset_timeout
Data type | UNS32
Data range | 100000 ≤ reset_timeout ≤ MAX(UNS32)
Axis types | T, R, S
Dimension | T: µs | R,S: µs
Default value | 0
Drive types | ----
Remarks |