# ID 70335

Function DIST_CTRL ON without SET_POS.
Description | Before distance control is activated, specify the command height of the workpiece surface SET_POS. Example: Z [DIST_CTRL ON SET_POS=100] See [FCT-M3// Section: Specifying the workpiece surface]
Response | Class | 7 | Immediate stop of the axis. The distance control is not enabled.
Solution | Class | 6 | Specify the set height of the workpiece surface SET_POS
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Block number [-]
Block number in the NC program where the error occurred.
Error type | 11, Error message from position controller.