# ID 110528

The parametrised controller dead band is bigger than the position window.
Description | The parameterised position controller dead band (P-AXIS-00395) is bigger than the position window (P-AXIS-00236) set for the axis.
Response | Class | 1 | Error message output, P-AXIS-00395 is limited to the value of P-AXIS-00236.
Solution | Class | 1 | Either reduce P-AXIS-00395 or increase P-AXIS-00236.
Parameter | %1: | Logical axis number [-]
Log. Axis number (see also P-AXIS-00016).
%2: | Incorrect value [0.1 µm or 0.0001°]
Value of P-AXIS-00395.
%3: | Limit value [0.1 µm or 0.0001°]
Value of P-AXIS-00236.
%4: | Corrected value [0.1 µm or 0.0001°]
Corrected value of P-AXIS-00395.
Error type | 2, Error message on data transfer of parameter lists to controller.