# ID 110606

Invalid combination of P-AXIS-00704 and P-AXIS-00261 configured.
Description | Axis parameters P-AXIS-00704 and P-AXIS-00261 were assigned contradictory values. If P-AXIS-00261 is set, only the values 'DEFAULT' or 'EDGE_TRIGGERED’ may be used for P-AXIS-00704.
Response | Class | 1 | Warning output, P-AXIS-00704 is set to 'EDGE_TRIGGERED'.
Solution | Class | 1 | If the edge detection of the 'gantry_on' signal is to be used, use the following setting: P-AXIS-00704 = 'EDGE_TRIGGERED' and P-AXIS-00261 = 0. When the edge detection is not to be used, set P-AXIS-00261 = 0 and, according to the desired function, either P-AXIS-00704 = 'DEFAULT' or P-AXIS-00704 = 'ONLY_CONTROL_UNIT'.
Parameter | %1: | Logical axis number [-]
Axis number
%2: | Current value [-]
Parameterized value of P-AXIS-00261.
%3: | Error value [-]
Parameterized value of P-AXIS-00704.
%4: | Corrected value [-]
Corrected value of P-AXIS-00261.
Error type | 2, Error message by data transfer from parameter list into control device.