# ID 60311

Specified filter time constant is invalid.
Description | The specified filter time constant P-AXIS-00357 is smaller or larger than permissible. The filter coefficients can therefore not be calculated. Permissible values are (with TAb = cycle time of the NC controller):

- For PT1 and PT2 filters:
  TAb ≤ P-AXIS-00357 ≤ MAX(UNS32)
- For time delay filters:
  0 ≤ P-AXIS-00357 < 6 * TAb

Response | Class | 3 | The filter is deactivated.
Solution | Class | 7 | Correct the parameter P-AXIS-00357
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis
%2: |
Number of concerned filter
%3: |
Filter typer P-AXIS-00204
%4: |
Invalid time constant P-AXIS-00357
%5: |
Maximum permissible time constant P-AXIS-00357
Error type | -