# ID 294022

legacy) drive error No. 91.
Description | The DSE-drive reports error No.91 (external error).
Response | Class | 7 | Stop the axis. All active commands inhibited.
Solution | Class | 6 | Contact the service personnel. Eliminate error. Reset the fault on the DSE-module.
Parameter | %1: |
Logical axis number P-AXIS-00016 of concerned axis.
%2: |
DSE drive address.
%3: |
DSE error id.
Error type | 11, Error message from position controller.