# Tube machining (#CYL ORI LATERAL)

## Notice

The kinematic parameters in ID 90 must be set for this machining type.

Syntax for selecting and parameterising, active as of the next motion block:

Syntax:
#CYL ORI LATERAL [ AX1<axis_name> | AXNR1=.. AX2<axis_name> | AXNR2=.. RADIUS=.. ]

AX1<axis_name> | Axis identifier of the first main axis (X or virtual linear axis U, flat projection)
AXNR1=.. | Logical axis number of first main axis (X or virtual linear axis U, flat projection), positive integer
AX2<axis_name> | Axis identifier of the second main axis (Y or virtual linear axis V, flat projection)
AXNR2=.. | Logical axis number of the second main axis (Y or virtual linear axis V, flat projection), positive integer
RADIUS=.. | Tube (bending) radius, [mm, inch]

Syntax for deselection:

#CYL OFF