# Centre point of a hole circle

The touch probe calculated the centre points of each of the drilled holes by 4 points (see SysMeasWcs8) and calculated the total centre point of the hole circle from the centre points.

The touch probe must be positioned as centrally as possible above the central point of the hole circle either manually or in automatic mode.

Centre point of a hole circle

## Additional information

- Process (internal cycle)
- Parameters
- Syntax
- Programming example
- Output variables