# ID 110335

Reduced Speed range limit neg. is smaller than neg. SLS.
Description | The negative range limit for Reduced Speed in the safety zones P-AXIS-00093, P-AXIS-00105 is smaller than the negative software limit switch. The negative range limit is set to the negative software limit switch position.
Response | Class | 1 | None.
Solution | Class | 1 | Select negative range limit greater than negative software limit switch.
Parameter | %1: | Logical axis number [0.1 µm or 0,0001°]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [0.1 µm or 0,0001°]
Current negative range limit.
%3: | Current value [0.1 µm or 0,0001°]
Negative software limit switch P-AXIS-00177.
%4: | Lower limit value [0.1 µm or 0,0001°]
Corrected negative range limit.
Error type | 2, Error message by data transfer from parameter list into control device.