# ID 20117

Double-programmed block transition.
Description | More than one G function from the group of block transition definitions (G60/G359/G360/G61/G260/G261) has been programmed in the same NC block. Example: Wrong: N10 G00 X0 Y0 Z0 N20 G360 X100 G60

:

N1000 M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible G function.
Parameter | %1: | Error value [-]
Number of the inadmissible programmed G function
Error type | 1, Error message from NC program.