# ID 110334

Reduced speed zone: upper range limit is greater than upper software limit switch.
Description | The positive range limit for Reduced Speed in the security zones P-AXIS-00085, P-AXIS-00097 is greater than the positive software limit switch. The positive range limit is set to the positive software limit switch position.
Response | Class | 1 | None.
Solution | Class | 1 | Select positive range limit smaller than positive software limit switch.
Parameter | %1: | Logical axis number [0.1 µm or 0.0001°]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [0.1 µm or 0.0001°]
Current positive range limit.
%3: | Upper limit value [0.1 µm or 0.0001°]
Positive software limit switch P-AXIS-00178.
%4: | Corrected value [0.1 µm or 0.0001°]
Corrected positive range limit.
Error type | 2, Error message on data transfer of parameter lists to controller.