# Error message suppression on reference loss of non-interpolated axes (P-AXIS-00825)

P-AXIS-00825 | Suppress error message on reference loss of non-interpolated axes
Description | When reference monitoring (antr.reference_check) is active, the error ID 70400 is output on loss of the reference position.. When P-AXIS-00825 is activated, this error can be suppressed. If the affected axes are interpolated when P-AXIS-00825 is set, the error ID 51082 is output.
Parameter | lr_param.suppress_reference_lost_error
Data type | BOOLEAN
Data range | 0: Error is not suppressed 1: Error is suppressed
Axis types | T, R, S
Dimension | T: --- | R,S: ---
Default value | 0
Drive types | SERCOS, CANopen
Remarks | Parameter available as of Builds V2.11.2070, V2.11.2841, V3.1.3080.17 or V3.1.3107.51