# ID 90202

Feed splitting not possible, programmed axis is not in the main plane.
Description | When the feed splitting function is used, the programmed axis is not in the main plane. The specified axis for feed splitting must be in the corresponding main plane. G17: XY plane (default) G18: ZX plane G19: YZ plane
Response | Class | 1 | Warning, no reaction., the feed is not split.
Solution | Class | 1 | Check and modify the specified axis
Parameter | %1: | Error value [-]
Logical axis number of the programmed axis
%2: | Expected value [-]
Logical axis number of the first axis of the main plane
%3: | Expected value [-]
Logical axis number of second axis of the main plane
%4: | Current value [-]
Select or deselect
Error type | 1, Error message from NC program.