# ID 21132

Double programming of spindle override.
Description | Error message occurs when programming the spindle override (G167). The override is programmed several times in the NC block for one spindle.
Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify the spindle programming within NC-block. Remove redundant G167 commands.
Error type | 1, Error message from NC program.