# ID 13102

Programmed machining depth exceeds permissible tool length.
Description | The maximum useful tool length can be entered in the tool parameters (see Section Cycle-specific tool data). In the case of a value unequal to zero, a check is made as to whether the programmed machining depth is less than the permissible usable tool length. If not, the message is generated.
Response | Class | - | Error: Transition to error state. Complete reset of the NC channel necessary.
Solution | Class | - | Check whether the permissible tool length is defined correctly. If necessary, use a different tool for machining with a tool length that is adequate for the machining depth.
Error type | Error message from NC cycle