# ID 110450

Modification of parameter p1042 requires a restart.
Description | Parameter P-AXIS-00316 cannot be changed while CNC kernel is running. The new value is not taken over, the previous active value remains valid.
Response | Class | 1 | None.
Solution | Class | 1 | Restart the controller after changing P-AXIS-00316.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [-]
Current value of P-AXIS-00316.
%3: | Corrected value [-]
Corrected (old) value of P-AXIS-00316.
Error type | 2, Error message by data transfer from parameter list into control device.