# ID 60196

Changeover velocity is greater than maximum feedrate.
Description | The changeover speed between acceleration levels 1 and 2 (P-AXIS-00221 or P-AXIS-00211) parameterized in the axis parameter list is greater than the permissible maximum speed of the axis P-AXIS-00212.
Response | Class | 1 | Warning output and value is corrected on P-AXIS-00212.
Solution | Class | 1 | Change axis parameter list, set P-AXIS-00221 or. P-AXIS-00211 smaller than P-AXIS-00212.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Current value [1µm/s or 0.001°/s]
Current parametrized value either P-AXIS-00211 or P-AXIS-00221.
%3: | Limit value [1µm/s or 0.001°/s]
Limit value (P-AXIS-00212)
%4: | Corrected value [1µm/s or 0.001°/s]
Corrected value
%5: | Current value [-]
This value specifies which parameter triggered the warning: 0: P-AXIS-00221 is faulty. 1: P-AXIS-00211 is faulty.
Error type | 1, Error message from NC program.