# ID 120470

No oscillation path.
Description | Invalid oscillation movement programmed. Wrong: %osc N10 X[OSC_ON 1ST_POS=50 2ND_POS=50 FEED=1000] N20 M30

Right:

%osc

N10 X[OSC_ON 1ST_POS=-100 2ND_POS=100 FEED=1000]

N20 M30

For more information on oscillation movement, see
[FCT-A8// Section: Description],
[PROG// Section: Oscillating axes].

Response | Class | 2 | Program execution stop.
Solution | Class | 6 | Check oscillation zero position and excursion, or oscillation reversal positions. There must be an oscillation path distance resulting from the difference between the oscillation reversal positions.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis.
%2: | Current value [0.1 µm or 0,0001°]
Oscillation reversal position 1.
%3: | Current value [0.1 µm or 0,0001°]
Oscillation reversal position 2.
Error type | 1, Error message from NC program.