# ID 20041

Motion information is required for MNE_SNS function.
Description | M functions of type MNE_SNS are triggered by an external event, and interrupt the current motion block accordingly. Therefore, they are not meaningful without a programmed motion information at the same time. Example: Wrong: M33 M30

Correct:

G01 X150 Y200 M33 F8

`M30`

Response | Class | 2 | Abort of the NC program processing.
Solution | Class | 3 | Check and modify NC program. Add a motion information.
Error type | 1, Error message from NC program. .