# ID 20430

Channel parameters: Number of groups exceeds maximum limit.
Description | At start-up, a check of the channel parameters detects that the total number of axis groups P-CHAN-00023 exceeds the permissible value range.
Response | Class | 1 | Controller start-up is continued.
Solution | Class | 1 | In case of conflict, the total number of axis groups at start-up is set to the maximum permissible limit value and the start-up is continued. Note: The complete number of configured axis groups in the channel parameter list may then not be available in the channel after start-up!

At the moment only one axis group (index 0) is permissible in NC channel.

Parameter | %1: | Current value [-]
Total number of axis groups P-CHAN-00023
%2: | Limit value [-]
Maximum permissible number of axis groups
%3: | Corrected value [-]
Total number of axis groups automatically corrected
Error type | 2, Error message by data transfer from parameter list into control device.