# ID 50706

End of movement range reached, measuring not executed.
Description | No measurement signal was enabled in one or more axes with measurement function G100 and the option of automated motion path limiting during measurement run (see P-CHAN-00268). The movement stops before reaching the movement range limits defined by the soft limit switch.

For detailed information on measurement function G100, see [FCT-C4],

[PROG// Section: Measuring functions].

Response | Class | 6 | Movement stop.
Solution | Class | 6 | Check measuring signal of the measurement axis/axes affected. Set measurement signal in all measurement axes with measurement interrupt.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of an affected measurement axis.
Error type | 1, Error message from NC program.