# ID 120471

Oscillating motion outside software limit switches.
Description | The programmed motion of the oscillating axis exceeds software limit switches. For more information on oscillating motion, see [FCT-A8// Section: Description [PROG// Section: Oscillating axes].
Response | Class | 2 | Program abort.
Solution | Class | 6 | Check oscillation zero position and excursion or the oscillation reversal positions. Program oscillating motion inside software limits.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected.
%2: | Current value [0.1 10^-3 mm or ø]
Oscillation reversal position 1.
%3: | Current value [0.1 10^-3 mm or ø]
Oscillation reversal position 2.
%4: | Lower limit value [0.1 10^-3 mm or ø]
Negative software limit switch P-AXIS-00177
%5: | Upper limit value [0.1 10^-3 mm or ø]
Positive software limit switch P-AXIS-00178
Error type | 1, Error message from NC program.