# ID 20115

Double-programmed diameter selection.
Description | More than one G function from the diameter programming group (G51/G52) has been programmed in the same NC block. Example: Wrong: N10 G90 G01 F1000 N20 G51 X80 G51

:

M30

Response | Class | 2 | Abort NC program processing.
Solution | Class | 3 | Check and modify NC program. Remove the inadmissible G function.
Parameter | %1: | Error value [-]
Number of the inadmissible programmed G function
Error type | 1, Error message from NC program.