# ID 120378

Changing the mode of HSC processing not permitted in active state.
Description | The HSC mode cannot be changed when the HSC function (#HSC[]) is active. For more information on the HSC function, see [PROG// Section: Standard HSC programming].
Response | Class | 2 | Program abort.
Solution | Class | 6 | Before changing the HSC mode, deselect the HSC function via #HSC[OFF].
Error type | 1, Error message from NC program.