# Number of axis groups (P-CHAN-00023)

P-CHAN-00023 | Number of axis groups in the NC channel
Description | This parameter defines the maximum number of axis groups.
Parameter | grp_anzahl
Data type | UNS16
Data range | 0 ... 1
Dimension | ----
Default value | 1
Remarks | Currently, only axis configurations are permitted with one axis group. This parameter must therefore always be assigned with '1'.