# Output of additional error information (P-STUP-00191)

P-STUP-00191 | Output of additional error information
Description | This text is forwarded transparently via the CNC_ERROR_INFO data structure if the filter condition applies, i.e. users have a possibility of conditionally also including additional error information in the output.
Parameter | error_filter[i].conditional_output where i = 0 ... 3 (maximum number of filters, application-specific)
Data type | STRING
Data range | Maximum 32 characters
Dimension | ----
Default value | *
Remarks | * Note: The default value of variables is a blank string.