# ID 70278

The #DRIVE command is not supported by this drive type.
Description | The #DRIVE command was used for an axis whose drive type does not support this command. See [PROG// Section: Drive-independent switching of drive functions]
Response | Class | 7 | Abort NC program.
Solution | Class | 6 | Change NC program.
Parameter | %1: | Logical axis number [-]
Logical axis number of affected axis see P-AXIS-00016
%2: | Logical axis number [-]
Drive type of the axis see P-AXIS-00020.
Error type | 11, Error message from position controller.