# ID 60240

Illegal bit combination commanded in CamIn start mode.
Description | When the PLC commanded a CamIn MC_CamIn), an invalid value for parameter ‘startmode’ was transferred to the PLC block.
Response | Class | 5 | PLC block reports an error.
Solution | Class | 6 | Change the ‘startmode’ call parameter of PLC block MC_CamIn.
Parameter | %1: |
Logical axis number (P-AXIS-00016) of the spindle
%2: | Error value [-]
Invalid value of ‘startmode’ parameter
%3: | Logical axis number [-]
Logical axis number of the master axis (P-AXIS-00016)
Error type | -