# ID 90165

Multipath programming not active when tool radius compensation is active.
Description | A NC program was started with TRC in 2 paths. The following parameters must be set in order to use TRC in 2 paths: Correct Channel parameter list: multi_path_configuration 1 # P-CHAN-00261

Activate the function:

configuration.tool_radius_comp.function MULTI_PATH # P-CHAN-00555

Alternatively, the function can be activated in the start-up list.

configuration.channel[0].tool_radius_comp.function MULTI_PATH # P-STUP-00080

Wrong:

configuration.tool_radius_comp.function 0

or in the start-up list

configuration.channel[0].tool_radius_comp.function 0

Response | Class | 2 | Abort NC program processing.
Solution | Class | 6 | Activate the function P-CHAN-00555 (or P-STUP-00080)
Error type | 1, Error message from NC program.