# ID 110218

Illegal grating of correction value intervals.
Description | The step size between 2 interpolation points from the list of compensation values for leadscrew error compensation is specified in parameter P-COMP-00018. The message is displayed because the value for the interval is < 0.
Response | Class | 3 | Correction of the value
Solution | Class | 7 | Check and modify the parameter P-COMP-00018. The value must be greater than 0.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of concerned axis
%2: | Error value [Incr.]
The CNC uses this value for parameter P-COMP-00009 instead of the value indicated by the user.
%3: | Lower limit value [Incr.]
Error type | 2, Error message by data transfer from parameter list into control device.