# ID 110588

The given relevant probing signal edge is invalid.
Description | Parameter P-AXIS-00518 "kenngr.measure.edge” defines the relevant probing signal edge for a measurement run (e.g. G100). However, the setting found is invalid. Correct values are POS (positive edge) or NEG (negative edge).
Response | Class | 1 | Warning and correct parameter P-AXIS-00517
Solution | Class | 1 | Correct the parameter P-AXIS-00518 for the relevant probing signal edge.
Parameter | %1: | Logical axis number [-]
Logical axis number P-AXIS-00016 of axis affected
%2: | Drive type [-]
Drive type P-AXIS-00020 of the axis
%3: | Current value [-]
Selected probing signal source P-AXIS-00516
%4: | Incorrect value [-]
Incorrect value for relevant probing signal edge P-AXIS-00518
%5: | Corrected value [-]
Corrected value for relevant probing signal edge P-AXIS-00518
Error type | 2, Error message on data transfer of parameter lists to controller.