# ID 110614

Parameter P-AXIS-00539 is not supported for this drive type.
Description | Parameter P-AXIS-00539 was assigned a value other than zero (nil), although the drive type used does not support this parameter.
Response | Class | 1 | Error message output, P-AXIS-00539 is set to zero (nil).
Solution | Class | 1 | P-AXIS-00539 shall be assigned the value zero (nil
Parameter | %1: | Logical axis number [-]
Log. Axis number
%2: | Drive type [-]
Drive type
%3: | Error value [-]
Incorrect value of P-AXIS-00539
%4: | Corrected value [-]
Corrected value of P-AXIS-00539
Error type | 2, Error message by data transfer from parameter list into control device.